MRT PCB

Power subsystems:

* 5 V power for RF electronics
* 9 V power for Arduino
* 15 V power for LNB
* 12 V power for motor controllers

Arduino:

* DIO to shift register to motor controller
* Low pass filter to ADC